CLARK S25CL
	Operational

	Load Capacity
	5,000 lb

	Load Center
	24 in

	Operator position
	Driver Seated



	Performance Data

	Travel Speed (Forward / Reverse) | Full Load
	11.2 mph

	Travel Speed (Forward / Reverse) | No Load
	11.5 mph

	Lifting Speed | Full Load
	102.4 fpm

	Lifting Speed | No Load
	106.3 fpm

	Lowering Speed | Full Load
	108.2 fpm

	Lowering Speed | No Load
	98.4 fpm

	Gradeability - Full load (3-minute ratings)
	33.8 %

	Gradeability - No load (3-minute ratings)
	18.8 %



	Truck weights

	Total Weight (Without Battery)
	8,380 lbs

	Weight Distribution - Full load (Front / Rear)
	11,383 lbs / 1,997 lbs

	Weight Distribution - No load (Front / Rear)
	2,822 lbs / 5,558 lbs



	Power system

	Power type
	L.P Gas

	Internal combustion engine - Make / Model
	FORD / FORD2.5

	Rated Horsepower @ rpm (SAE)
	69.7 hp @ 2,500rpm

	Number of Cylinders
	4

	Piston Displacement
	152 cu in

	Sound level (Measured per ANSI B56.11.5)
	79 dB



	Mast specification

	Maximum Lift Height (1st stage mast)
	83 in (Min) - 204 in (Max)

	Maximum Lift Height (2nd stage mast)
	240 in (Min) - 312 in (Max)

	Maximum Lift Height (3rd stage mast)
	115 in (Min) - 244 in (Max)

	Maximum Lift Height (4th stage mast)
	240 in (Min) - 312 in (Max)



	Exterior dimensions

	Free-Lift (top of forks)
	4.3 in

	Maximum Lift Height
	130 in

	Fork Size (T x W x L)
	1.75 x 4 x 42 in

	Tilt Range (forward / backward)
	8 / 10 deg

	Overall Length
	134.4 in

	Length to Fork Face
	92.3 in

	Mast Lowered Height
	83.3 in

	Mast Extended Height (top of load backrest)
	151.7 in

	Overhead Guard Height
	82.9 in

	Turning Radius (outside)
	81.1 in

	Turning Radius (Internal)
	21.5 in

	Load Distance (Center of wheel to face of forks)
	16.1 in

	Basic Right-Angle Stack
	97.2 in

	Carriage Width
	37 in

	Wheelbase
	56.3 in

	Underclearance - Minimum (mast)
	3.3 in

	Underclearance - Center of Wheelbase
	4.3 in

	Tow pin height (Vertical center of pin)
	12.2 in

	Seat height (from floor to Seat-in-Place)
	43.8 in

	Tread width (Front / Rear)
	34.8 in / 35.2 in

	Grade clearance
	50 %



	Tires

	Type (Front)
	Cushion

	Type (Rear)
	Cushion

	Type (Caster)
	Cushion

	Wheels (x=driven) - Front/rear
	2x / 2

	Tire Size (Front)
	21x7 in

	Tire Size (Rear)
	16x5-10.5 in

	Brake (Service)
	WET



