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· Axle-Front: High Bias, Limited Slip
· Axle-Rear: Planetary
· Capacity – Fuel Tank: 38 gal. / 143.85 L
· Drawbar Pull: 24000 lb / 10886.22 kg
· Engine Horsepower: 130 hp / 96.98 kW
· Engine Manufacturer: Cummins
· Engine Model: QSB4.5L ATAAC Tier 4 Interim
· Frame Leveling: 10 Degrees
· Function Pump Type: Load Sensing Piston
· Ground Clearance: 1 ft 6 in. / 0.46 m
· Lift Capacity at Full Height: 7000 lb / 3175.15 kg
· Lift Capacity at Max Reach (Stabs Up): 2000 lb / 907.18 kg
· Load Center: 2 ft / 0.61 m
· Machine Height: 8 ft 5 in. / 2.57 m
· Machine Length: 20 ft / 6.1 m
· Machine Width: 8 ft 5 in. / 2.57 m
· Maximum Engine RPM: 1500 rpm
· Maximum Lift Capacity: 15000 lb / 6803.89 kg
· Maximum Lift Height: 44 ft / 13.41 m
· Maximum Reach: 31 ft / 9.45 m
· Operating Vehicle Weight: 32500 lb / 14741.75 kg
· Outriggers or Stabilizers: No
· Outside Turning Radius: 14 ft 6 in. / 4.42 m
· Service Brake Type: Wet Multi-Disc
· Speed – Maximum Lift: 16 sec.
· Speed – Maximum Lower: 15 sec.
· Speed – Maximum Telescope In: 13 sec.
· Speed – Maximum Telescope Out: 17 sec.
· Speed – Maximum Travel: 20 mph / 32.19 km/h
· Tire Size: 17.5 x 25
· Transmission – Nr Forward Gears Standard: 4
· Transmission – Nr Reverse Gears: 3
· Transmission Type: Powershift
· Wheelbase: 12 ft / 3.66 m
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